{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["tab1","tab2"],"not_rendered":{"charts":1,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"tab1","index":0,"n_rows":1,"n_cols":1,"rows_kept":1,"cut":false,"hidden":false,"merged":[]}
["Title page"]

{"sheet":"tab2","index":1,"n_rows":24,"n_cols":5,"rows_kept":24,"cut":false,"hidden":false,"merged":[[10,0,10,1],[0,0,0,6],[3,0,3,1],[3,3,3,4],[2,0,2,4]]}
["This workbook calculates the average delay using the equation da=(0.5r(1-g/C))/(1-v/s)"]
[]
["Task 1"]
["Inputs",null,null,"Output"]
["r",{"$f":"0.5*B7","v":20},null,"Average Delay (s)",{"$f":"da(B5,B6,B7,B8,B9)","v":9.4999999999999982}]
["g",{"$f":"B5","v":20}]
["C",40]
["v",900]
["s",1900]
[]
["Task 2"]
["Cycle Length (s)","Average Delay (s)"]
[40,10]
[50,12.5]
[60,15]
[70,17.5]
[80,20]
[90,22.5]
[100,25]
[110,27.5]
[120,30]
[130,32.5]
[140,35]
[150,37.5]