# ECE 341 Lab 2 Prelab Questions

1. What will affect how close your pure software delay can get to 1 ms resolution?
2. What do you see as the advantages of the hardware-assisted delay method?
3. What is the “range” of each method, i.e. the minimum and maximum delay?